# Section XV Base metals and articles of base metal

## Chapter 72 Iron and Steel

| Commodity code | Duty expression | Notes | Description |
| --- | --- | --- | --- |
| **7200** |  |  | **IRON AND STEEL** |
|  |  |  | **I. PRIMARY MATERIALS; PRODUCTS IN GRANULAR OR POWDER FORM** |
| **7201** |  |  | **Pig iron and spiegeleisen in pigs, blocks or other primary forms** |
| **7201 10** |  |  | - Non-alloy pig iron containing by weight 0.5% or less of phosphorus |
|  |  |  | - - Containing by weight not less than 0.4% of manganese |
| **7201 10 11** | 0.0% |  | - - - Containing by weight 1% or less of silicon |
| **7201 10 19** | 0.0% |  | - - - Containing by weight more than 1% of silicon |
| **7201 10 30** | 0.0% |  | - - Containing by weight not less than 0.1% but less than 0.4% of manganese |
| **7201 10 90** | 0.0% |  | - - Containing by weight less than 0.1% of manganese |
| **7201 20** | 0.0% |  | - Non-alloy pig iron containing by weight more than 0.5% of phosphorus |
| **7201 50** |  |  | - Alloy pig iron; spiegeleisen |
| **7201 50 10** | 0.0% |  | - - Alloy pig iron containing by weight not less than 0.3% but not more than 1% of titanium and not less than 0.5% but not more than 1% of vanadium |
| **7201 50 90** | 0.0% |  | - - Other |
| **7202** |  |  | **Ferro-alloys** |
|  |  |  | - Ferro-manganese |
| **7202 11** |  |  | - - Containing by weight more than 2% of carbon |
| **7202 11 20** | 0.0% |  | - - - With a granulometry not exceeding 5 mm and a manganese content by weight exceeding 65% |
| **7202 11 80** | 0.0% |  | - - - Other |
| **7202 19** | 0.0% |  | - - Other |
|  |  |  | - Ferro-silicon |
| **7202 21** | 0.0% |  | - - Containing by weight more than 55% of silicon |
| **7202 29** |  |  | - - Other |
| **7202 29 10** | 0.0% |  | - - - Containing by weight 4% or more but not more than 10% of magnesium |
| **7202 29 90** | 0.0% |  | - - - Other |
| **7202 30** | 0.0% |  | - Ferro-silico-manganese |
|  |  |  | - Ferro-chromium |
| **7202 41** |  |  | - - Containing by weight more than 4% of carbon |
| **7202 41 10** | 0.0% |  | - - - Containing by weight more than 4% but not more than 6% of carbon |
| **7202 41 90** | 0.0% |  | - - - Containing by weight more than 6% of carbon |
| **7202 49** |  |  | - - Other |
| **7202 49 10** | 0.0% |  | - - - Containing by weight not more than 0.05% of carbon |
| **7202 49 50** | 0.0% |  | - - - Containing by weight more than 0.05% but not more than 0.5% of carbon |
| **7202 49 90** | 0.0% |  | - - - Containing by weight more than 0.5% but not more than 4% of carbon |
| **7202 50** | 0.0% |  | - Ferro-silico-chromium |
| **7202 60** | 0.0% |  | - Ferro-nickel |
| **7202 70** | 0.0% |  | - Ferro-molybdenum |
| **7202 80** | 0.0% |  | - Ferro-tungsten and ferro-silico-tungsten |
|  |  |  | - Other |
| **7202 91** | 0.0% |  | - - Ferro-titanium and ferro-silico-titanium |
| **7202 92** | 0.0% |  | - - Ferro-vanadium |
| **7202 93** | 0.0% |  | - - Ferro-niobium |
| **7202 99** |  |  | - - Other |
| **7202 99 10** | 0.0% |  | - - - Ferro-phosphorus |
| **7202 99 30** | 0.0% |  | - - - Ferro-silico-magnesium |
| **7202 99 80** | 0.0% |  | - - - Other |
| **7203** |  |  | **Ferrous products obtained by direct reduction of iron ore and other spongy ferrous products, in lumps, pellets or similar forms; iron having a minimum purity by weight of 99.94%, in lumps, pellets or similar forms** |
| **7203 10** | 0.0% |  | - Ferrous products obtained by direct reduction of iron ore |
| **7203 90** | 0.0% |  | - Other |
| **7204** |  |  | **Ferrous waste and scrap; remelting scrap ingots of iron or steel** |
| **7204 10** | 0.0% |  | - Waste and scrap of cast iron |
|  |  |  | - Waste and scrap of alloy steel |
| **7204 21** |  |  | - - Of stainless steel |
| **7204 21 10** | 0.0% |  | - - - Containing by weight 8% or more of nickel |
| **7204 21 90** | 0.0% |  | - - - Other |
| **7204 29** | 0.0% |  | - - Other |
| **7204 30** | 0.0% |  | - Waste and scrap of tinned iron or steel |
|  |  |  | - Other waste and scrap |
| **7204 41** |  |  | - - Turnings, shavings, chips, milling waste, sawdust, filings, trimmings and stampings, whether or not in bundles |
| **7204 41 10** | 0.0% |  | - - - Turnings, shavings, chips, milling waste, sawdust and filings |
|  |  |  | - - - Trimmings and stampings |
| **7204 41 91** | 0.0% |  | - - - - In bundles |
| **7204 41 99** | 0.0% |  | - - - - Other |
| **7204 49** |  |  | - - Other |
| **7204 49 10** | 0.0% |  | - - - Fragmentised (shredded) |
|  |  |  | - - - Other |
| **7204 49 30** | 0.0% |  | - - - - In bundles |
| **7204 49 90** | 0.0% |  | - - - - Other |
| **7204 50** | 0.0% |  | - Remelting scrap ingots |
| **7205** |  |  | **Granules and powders, of pig iron, spiegeleisen, iron or steel** |
| **7205 10** | 0.0% |  | - Granules |
|  |  |  | - Powders |
| **7205 21** | 0.0% |  | - - Of alloy steel |
| **7205 29** | 0.0% |  | - - Other |
|  |  |  | **II. IRON AND NON-ALLOY STEEL** |
| **7206** |  |  | **Iron and non-alloy steel in ingots or other primary forms (excluding iron of heading 7203)** |
| **7206 10** | 0.0% |  | - Ingots |
| **7206 90** | 0.0% |  | - Other |
| **7207** |  |  | **Semi-finished products of iron or non-alloy steel** |
|  |  |  | - Containing by weight less than 0.25% of carbon |
| **7207 11** |  |  | - - Of rectangular (including square) cross-section, the width measuring less than twice the thickness |
|  |  |  | - - - Rolled or obtained by continuous casting |
| **7207 11 11** | 0.0% |  | - - - - Of free-cutting steel |
|  |  |  | - - - - Other |
| **7207 11 14** | 0.0% |  | - - - - - Of a thickness not exceeding 130 mm |
| **7207 11 16** | 0.0% |  | - - - - - Of a thickness exceeding 130 mm |
| **7207 11 90** | 0.0% |  | - - - Forged |
| **7207 12** |  |  | - - Other, of rectangular (other than square) cross-section |
| **7207 12 10** | 0.0% |  | - - - Rolled or obtained by continuous casting |
| **7207 12 90** | 0.0% |  | - - - Forged |
| **7207 19** |  |  | - - Other |
|  |  |  | - - - Of circular or polygonal cross-section |
| **7207 19 12** | 0.0% |  | - - - - Rolled or obtained by continuous casting |
| **7207 19 19** | 0.0% |  | - - - - Forged |
| **7207 19 80** | 0.0% |  | - - - Other |
| **7207 20** |  |  | - Containing by weight 0.25% or more of carbon |
|  |  |  | - - Of rectangular (including square) cross-section, the width measuring less than twice the thickness |
|  |  |  | - - - Rolled or obtained by continuous casting |
| **7207 20 11** | 0.0% |  | - - - - Of free-cutting steel |
|  |  |  | - - - - Other, containing by weight |
| **7207 20 15** | 0.0% |  | - - - - - 0,25% or more but less than 0.6% of carbon |
| **7207 20 17** | 0.0% |  | - - - - - 0.6% or more of carbon |
| **7207 20 19** | 0.0% |  | - - - Forged |
|  |  |  | - - Other, of rectangular (other than square) cross-section |
| **7207 20 32** | 0.0% |  | - - - Rolled or obtained by continuous casting |
| **7207 20 39** | 0.0% |  | - - - Forged |
|  |  |  | - - Of circular or polygonal cross-section |
| **7207 20 52** | 0.0% |  | - - - Rolled or obtained by continuous casting |
| **7207 20 59** | 0.0% |  | - - - Forged |
| **7207 20 80** | 0.0% |  | - - Other |
| **7208** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of 600 mm or more, hot-rolled, not clad, plated or coated** |
| **7208 10** | 0.0% |  | - In coils, not further worked than hot-rolled, with patterns in relief |
|  |  |  | - Other, in coils, not further worked than hot-rolled, pickled |
| **7208 25** | 0.0% |  | - - Of a thickness of 4.75 mm or more |
| **7208 26** | 0.0% |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7208 27** | 0.0% |  | - - Of a thickness of less than 3 mm |
|  |  |  | - Other, in coils, not further worked than hot-rolled |
| **7208 36** | 0.0% |  | - - Of a thickness exceeding 10 mm |
| **7208 37** | 0.0% |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7208 38** | 0.0% |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7208 39** | 0.0% |  | - - Of a thickness of less than 3 mm |
| **7208 40** | 0.0% |  | - Not in coils, not further worked than hot-rolled, with patterns in relief |
|  |  |  | - Other, not in coils, not further worked than hot-rolled |
| **7208 51** |  |  | - - Of a thickness exceeding 10 mm |
| **7208 51 20** | 0.0% |  | - - - Of a thickness exceeding 15 mm |
|  |  |  | - - - Of a thickness exceeding 10 mm but not exceeding 15 mm, of a width of |
| **7208 51 91** | 0.0% |  | - - - - 2 050 mm or more |
| **7208 51 98** | 0.0% |  | - - - - Less than 2 050 mm |
| **7208 52** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7208 52 10** | 0.0% |  | - - - Rolled on four faces or in a closed box pass, of a width not exceeding 1 250 mm |
|  |  |  | - - - Other, of a width of |
| **7208 52 91** | 0.0% |  | - - - - 2 050 mm or more |
| **7208 52 99** | 0.0% |  | - - - - Less than 2 050 mm |
| **7208 53** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7208 53 10** | 0.0% |  | - - - Rolled on four faces or in a closed box pass, of a width not exceeding 1 250 mm and of a thickness of 4 mm or more |
| **7208 53 90** | 0.0% |  | - - - Other |
| **7208 54** | 0.0% |  | - - Of a thickness of less than 3 mm |
| **7208 90** |  |  | - Other |
| **7208 90 20** | 0.0% |  | - - Perforated |
| **7208 90 80** | 0.0% |  | - - Other |
| **7209** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of 600 mm or more, cold-rolled (cold-reduced), not clad, plated or coated** |
|  |  |  | - In coils, not further worked than cold-rolled (cold-reduced) |
| **7209 15** | 0.0% |  | - - Of a thickness of 3 mm or more |
| **7209 16** |  |  | - - Of a thickness exceeding 1 mm but less than 3 mm |
| **7209 16 10** | 0.0% |  | - - - 'Electrical' |
| **7209 16 90** | 0.0% |  | - - - Other |
| **7209 17** |  |  | - - Of a thickness of 0.5 mm or more but not exceeding 1 mm |
| **7209 17 10** | 0.0% |  | - - - 'Electrical' |
| **7209 17 90** | 0.0% |  | - - - Other |
| **7209 18** |  |  | - - Of a thickness of less than 0.5 mm |
| **7209 18 10** | 0.0% |  | - - - 'Electrical' |
|  |  |  | - - - Other |
| **7209 18 91** | 0.0% |  | - - - - Of a thickness of 0.35 mm or more but less than 0.5 mm |
| **7209 18 99** | 0.0% |  | - - - - Of a thickness of less than 0.35 mm |
|  |  |  | - Not in coils, not further worked than cold-rolled (cold-reduced) |
| **7209 25** | 0.0% |  | - - Of a thickness of 3 mm or more |
| **7209 26** |  |  | - - Of a thickness exceeding 1 mm but less than 3 mm |
| **7209 26 10** | 0.0% |  | - - - 'Electrical' |
| **7209 26 90** | 0.0% |  | - - - Other |
| **7209 27** |  |  | - - Of a thickness of 0.5 mm or more but not exceeding 1 mm |
| **7209 27 10** | 0.0% |  | - - - 'Electrical' |
| **7209 27 90** | 0.0% |  | - - - Other |
| **7209 28** |  |  | - - Of a thickness of less than 0.5 mm |
| **7209 28 10** | 0.0% |  | - - - 'Electrical' |
| **7209 28 90** | 0.0% |  | - - - Other |
| **7209 90** |  |  | - Other |
| **7209 90 20** | 0.0% |  | - - Perforated |
| **7209 90 80** | 0.0% |  | - - Other |
| **7210** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of 600 mm or more, clad, plated or coated** |
|  |  |  | - Plated or coated with tin |
| **7210 11** | 0.0% |  | - - Of a thickness of 0.5 mm or more |
| **7210 12** |  |  | - - Of a thickness of less than 0.5 mm |
| **7210 12 20** | 0.0% |  | - - - Tinplate |
| **7210 12 80** | 0.0% |  | - - - Other |
| **7210 20** | 0.0% |  | - Plated or coated with lead, including terne-plate |
| **7210 30** | 0.0% |  | - Electrolytically plated or coated with zinc |
|  |  |  | - Otherwise plated or coated with zinc |
| **7210 41** | 0.0% |  | - - Corrugated |
| **7210 49** | 0.0% |  | - - Other |
| **7210 50** | 0.0% |  | - Plated or coated with chromium oxides or with chromium and chromium oxides |
|  |  |  | - Plated or coated with aluminium |
| **7210 61** | 0.0% |  | - - Plated or coated with aluminium-zinc alloys |
| **7210 69** | 0.0% |  | - - Other |
| **7210 70** |  |  | - Painted, varnished or coated with plastics |
| **7210 70 10** | 0.0% |  | - - Tinplate, varnished; products, plated or coated with chromium oxides or with chromium and chromium oxides, varnished |
| **7210 70 80** | 0.0% |  | - - Other |
| **7210 90** |  |  | - Other |
| **7210 90 30** | 0.0% |  | - - Clad |
| **7210 90 40** | 0.0% |  | - - Tinned and printed |
| **7210 90 80** | 0.0% |  | - - Other |
| **7211** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of less than 600 mm, not clad, plated or coated** |
|  |  |  | - Not further worked than hot-rolled |
| **7211 13** | 0.0% |  | - - Rolled on four faces or in a closed box pass, of a width exceeding 150 mm and a thickness of not less than 4 mm, not in coils and without patterns in relief |
| **7211 14** | 0.0% |  | - - Other, of a thickness of 4.75 mm or more |
| **7211 19** | 0.0% |  | - - Other |
|  |  |  | - Not further worked than cold-rolled (cold-reduced) |
| **7211 23** |  |  | - - Containing by weight less than 0.25% of carbon |
| **7211 23 20** | 0.0% |  | - - - 'Electrical' |
|  |  |  | - - - Other |
| **7211 23 30** | 0.0% |  | - - - - Of a thickness of 0.35 mm or more |
| **7211 23 80** | 0.0% |  | - - - - Of a thickness of less than 0.35 mm |
| **7211 29** | 0.0% |  | - - Other |
| **7211 90** |  |  | - Other |
| **7211 90 20** | 0.0% |  | - - Perforated |
| **7211 90 80** | 0.0% |  | - - Other |
| **7212** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of less than 600 mm, clad, plated or coated** |
| **7212 10** |  |  | - Plated or coated with tin |
| **7212 10 10** | 0.0% |  | - - Tinplate, not further worked than surface-treated |
| **7212 10 90** | 0.0% |  | - - Other |
| **7212 20** | 0.0% |  | - Electrolytically plated or coated with zinc |
| **7212 30** | 0.0% |  | - Otherwise plated or coated with zinc |
| **7212 40** |  |  | - Painted, varnished or coated with plastics |
| **7212 40 20** | 0.0% |  | - - Tinplate, not further worked than varnished; products, plated or coated with chromium oxides or with chromium and chromium oxides, varnished |
| **7212 40 80** | 0.0% |  | - - Other |
| **7212 50** |  |  | - Otherwise plated or coated |
| **7212 50 20** | 0.0% |  | - - Plated or coated with chromium oxides or with chromium and chromium oxides |
| **7212 50 30** | 0.0% |  | - - Plated or coated with chromium or nickel |
| **7212 50 40** | 0.0% |  | - - Plated or coated with copper |
|  |  |  | - - Plated or coated with aluminium |
| **7212 50 61** | 0.0% |  | - - - Plated or coated with aluminium-zinc alloys |
| **7212 50 69** | 0.0% |  | - - - Other |
| **7212 50 90** | 0.0% |  | - - Other |
| **7212 60** | 0.0% |  | - Clad |
| **7213** |  |  | **Bars and rods, hot-rolled, in irregularly wound coils, of iron or non-alloy steel** |
| **7213 10** | 0.0% |  | - Containing indentations, ribs, grooves or other deformations produced during the rolling process |
| **7213 20** | 0.0% |  | - Other, of free-cutting steel |
|  |  |  | - Other |
| **7213 91** |  |  | - - Of circular cross-section measuring less than 14 mm in diameter |
| **7213 91 10** | 0.0% |  | - - - Of a type used for concrete reinforcement |
| **7213 91 20** | 0.0% |  | - - - Of a type used for tyre cord |
|  |  |  | - - - Other |
| **7213 91 41** | 0.0% |  | - - - - Containing by weight 0.06% or less of carbon |
| **7213 91 49** | 0.0% |  | - - - - Containing by weight more than 0.06% but less than 0.25% of carbon |
| **7213 91 70** | 0.0% |  | - - - - Containing by weight 0.25% or more but not more than 0.75% of carbon |
| **7213 91 90** | 0.0% |  | - - - - Containing by weight more than 0.75% of carbon |
| **7213 99** |  |  | - - Other |
| **7213 99 10** | 0.0% |  | - - - Containing by weight less than 0.25% of carbon |
| **7213 99 90** | 0.0% |  | - - - Containing by weight 0.25% or more of carbon |
| **7214** |  |  | **Other bars and rods of iron or non-alloy steel, not further worked than forged, hot-rolled, hot-drawn or hot-extruded, but including those twisted after rolling** |
| **7214 10** | 0.0% |  | - Forged |
| **7214 20** | 0.0% |  | - Containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7214 30** | 0.0% |  | - Other, of free-cutting steel |
|  |  |  | - Other |
| **7214 91** |  |  | - - Of rectangular (other than square) cross-section |
| **7214 91 10** | 0.0% |  | - - - Containing by weight less than 0.25% of carbon |
| **7214 91 90** | 0.0% |  | - - - Containing by weight 0.25% or more of carbon |
| **7214 99** |  |  | - - Other |
|  |  |  | - - - Containing by weight less than 0.25% of carbon |
| **7214 99 10** | 0.0% |  | - - - - Of a type used for concrete reinforcement |
|  |  |  | - - - - Other, of circular cross-section measuring in diameter |
| **7214 99 31** | 0.0% |  | - - - - - 80 mm or more |
| **7214 99 39** | 0.0% |  | - - - - - Less than 80 mm |
| **7214 99 50** | 0.0% |  | - - - - Other |
|  |  |  | - - - Containing by weight 0.25% or more of carbon |
|  |  |  | - - - - Of a circular cross-section measuring in diameter |
| **7214 99 71** | 0.0% |  | - - - - - 80 mm or more |
| **7214 99 79** | 0.0% |  | - - - - - Less than 80 mm |
| **7214 99 95** | 0.0% |  | - - - - Other |
| **7215** |  |  | **Other bars and rods of iron or non-alloy steel** |
| **7215 10** | 0.0% |  | - Of free-cutting steel, not further worked than cold-formed or cold-finished |
| **7215 50** |  |  | - Other, not further worked than cold-formed or cold-finished |
|  |  |  | - - Containing by weight less than 0.25% of carbon |
| **7215 50 11** | 0.0% |  | - - - Of rectangular (other than square) cross-section |
| **7215 50 19** | 0.0% |  | - - - Other |
| **7215 50 80** | 0.0% |  | - - Containing by weight 0.25% or more of carbon |
| **7215 90** | 0.0% |  | - Other |
| **7216** |  |  | **Angles, shapes and sections of iron or non-alloy steel** |
| **7216 10** | 0.0% |  | - U, I or H sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of less than 80 mm |
|  |  |  | - L or T sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of less than 80 mm |
| **7216 21** | 0.0% |  | - - L sections |
| **7216 22** | 0.0% |  | - - T sections |
|  |  |  | - U, I or H sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of 80 mm or more |
| **7216 31** |  |  | - - U sections |
| **7216 31 10** | 0.0% |  | - - - Of a height of 80 mm or more but not exceeding 220 mm |
| **7216 31 90** | 0.0% |  | - - - Of a height exceeding 220 mm |
| **7216 32** |  |  | - - I sections |
|  |  |  | - - - Of a height of 80 mm or more but not exceeding 220 mm |
| **7216 32 11** | 0.0% |  | - - - - With parallel flange faces |
| **7216 32 19** | 0.0% |  | - - - - Other |
|  |  |  | - - - Of a height exceeding 220 mm |
| **7216 32 91** | 0.0% |  | - - - - With parallel flange faces |
| **7216 32 99** | 0.0% |  | - - - - Other |
| **7216 33** |  |  | - - H sections |
| **7216 33 10** | 0.0% |  | - - - Of a height of 80 mm or more but not exceeding 180 mm |
| **7216 33 90** | 0.0% |  | - - - Of a height exceeding 180 mm |
| **7216 40** |  |  | - L or T sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of 80 mm or more |
| **7216 40 10** | 0.0% |  | - - L sections |
| **7216 40 90** | 0.0% |  | - - T sections |
| **7216 50** |  |  | - Other angles, shapes and sections, not further worked than hot-rolled, hot-drawn or extruded |
| **7216 50 10** | 0.0% |  | - - With a cross-section which is capable of being enclosed in a square the side of which is 80 mm |
|  |  |  | - - Other |
| **7216 50 91** | 0.0% |  | - - - Bulb flats |
| **7216 50 99** | 0.0% |  | - - - Other |
|  |  |  | - Angles, shapes and sections, not further worked than cold-formed or cold-finished |
| **7216 61** |  |  | - - Obtained from flat-rolled products |
| **7216 61 10** | 0.0% |  | - - - C, L, U, Z, omega or open-ended sections |
| **7216 61 90** | 0.0% |  | - - - Other |
| **7216 69** | 0.0% |  | - - Other |
|  |  |  | - Other |
| **7216 91** |  |  | - - Cold-formed or cold-finished from flat-rolled products |
| **7216 91 10** | 0.0% |  | - - - Profiled (ribbed) sheets |
| **7216 91 80** | 0.0% |  | - - - Other |
| **7216 99** | 0.0% |  | - - Other |
| **7217** |  |  | **Wire of iron or non-alloy steel** |
| **7217 10** |  |  | - Not plated or coated, whether or not polished |
|  |  |  | - - Containing by weight less than 0.25% of carbon |
| **7217 10 10** | 0.0% |  | - - - With a maximum cross-sectional dimension of less than 0.8 mm |
|  |  |  | - - - With a maximum cross-sectional dimension of 0.8 mm or more |
| **7217 10 31** | 0.0% |  | - - - - Containing indentations, ribs, grooves or other deformations produced during the rolling process |
| **7217 10 39** | 0.0% |  | - - - - Other |
| **7217 10 50** | 0.0% |  | - - Containing by weight 0.25% or more but less than 0.6% of carbon |
| **7217 10 90** | 0.0% |  | - - Containing by weight 0.6% or more of carbon |
| **7217 20** |  |  | - Plated or coated with zinc |
|  |  |  | - - Containing by weight less than 0.25% of carbon |
| **7217 20 10** | 0.0% |  | - - - With a maximum cross-sectional dimension of less than 0.8 mm |
| **7217 20 30** | 0.0% |  | - - - With a maximum cross-sectional dimension of 0.8 mm or more |
| **7217 20 50** | 0.0% |  | - - Containing by weight 0.25% or more but less than 0.6% of carbon |
| **7217 20 90** | 0.0% |  | - - Containing by weight 0.6% or more of carbon |
| **7217 30** |  |  | - Plated or coated with other base metals |
|  |  |  | - - Containing by weight less than 0.25% of carbon |
| **7217 30 41** | 0.0% |  | - - - Copper-coated |
| **7217 30 49** | 0.0% |  | - - - Other |
| **7217 30 50** | 0.0% |  | - - Containing by weight 0.25% or more but less than 0.6% of carbon |
| **7217 30 90** | 0.0% |  | - - Containing by weight 0.6% or more of carbon |
| **7217 90** |  |  | - Other |
| **7217 90 20** | 0.0% |  | - - Containing by weight less than 0.25% of carbon |
| **7217 90 50** | 0.0% |  | - - Containing by weight 0.25% or more but less than 0.6% of carbon |
| **7217 90 90** | 0.0% |  | - - Containing by weight 0.6% or more of carbon |
|  |  |  | **III. STAINLESS STEEL** |
| **7218** |  |  | **Stainless steel in ingots or other primary forms; semi-finished products of stainless steel** |
| **7218 10** | 0.0% |  | - Ingots and other primary forms |
|  |  |  | - Other |
| **7218 91** |  |  | - - Of rectangular (other than square) cross-section |
| **7218 91 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7218 91 80** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7218 99** |  |  | - - Other |
|  |  |  | - - - Of square cross-section |
| **7218 99 11** | 0.0% |  | - - - - Rolled or obtained by continuous casting |
| **7218 99 19** | 0.0% |  | - - - - Forged |
|  |  |  | - - - Other |
| **7218 99 20** | 0.0% |  | - - - - Rolled or obtained by continuous casting |
| **7218 99 80** | 0.0% |  | - - - - Forged |
| **7219** |  |  | **Flat-rolled products of stainless steel, of a width of 600 mm or more** |
|  |  |  | - Not further worked than hot-rolled, in coils |
| **7219 11** | 0.0% |  | - - Of a thickness exceeding 10 mm |
| **7219 12** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7219 12 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 12 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 13** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7219 13 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 13 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 14** |  |  | - - Of a thickness of less than 3 mm |
| **7219 14 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 14 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
|  |  |  | - Not further worked than hot-rolled, not in coils |
| **7219 21** |  |  | - - Of a thickness exceeding 10 mm |
| **7219 21 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 21 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 22** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7219 22 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 22 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 23** | 0.0% |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7219 24** | 0.0% |  | - - Of a thickness of less than 3 mm |
|  |  |  | - Not further worked than cold-rolled (cold-reduced) |
| **7219 31** | 0.0% |  | - - Of a thickness of 4.75 mm or more |
| **7219 32** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7219 32 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 32 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 33** |  |  | - - Of a thickness exceeding 1 mm but less than 3 mm |
| **7219 33 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 33 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 34** |  |  | - - Of a thickness of 0.5 mm or more but not exceeding 1 mm |
| **7219 34 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 34 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 35** |  |  | - - Of a thickness of less than 0.5 mm |
| **7219 35 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7219 35 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7219 90** |  |  | - Other |
| **7219 90 20** | 0.0% |  | - - Perforated |
| **7219 90 80** | 0.0% |  | - - Other |
| **7220** |  |  | **Flat-rolled products of stainless steel, of a width of less than 600 mm** |
|  |  |  | - Not further worked than hot-rolled |
| **7220 11** | 0.0% |  | - - Of a thickness of 4.75 mm or more |
| **7220 12** | 0.0% |  | - - Of a thickness of less than 4.75 mm |
| **7220 20** |  |  | - Not further worked than cold-rolled (cold-reduced) |
|  |  |  | - - Of a thickness of 3 mm or more, containing by weight |
| **7220 20 21** | 0.0% |  | - - - 2.5% or more of nickel |
| **7220 20 29** | 0.0% |  | - - - Less than 2.5% of nickel |
|  |  |  | - - Of a thickness exceeding 0.35 mm but of less than 3 mm, containing by weight |
| **7220 20 41** | 0.0% |  | - - - 2.5% or more of nickel |
| **7220 20 49** | 0.0% |  | - - - Less than 2.5% of nickel |
|  |  |  | - - Of a thickness not exceeding 0.35 mm, containing by weight |
| **7220 20 81** | 0.0% |  | - - - 2.5% or more of nickel |
| **7220 20 89** | 0.0% |  | - - - Less than 2.5% of nickel |
| **7220 90** |  |  | - Other |
| **7220 90 20** | 0.0% |  | - - Perforated |
| **7220 90 80** | 0.0% |  | - - Other |
| **7221** |  |  | **Bars and rods, hot-rolled, in irregularly wound coils, of stainless steel** |
| **7221 00 10** | 0.0% |  | - Containing by weight 2.5% or more of nickel |
| **7221 00 90** | 0.0% |  | - Containing by weight less than 2.5% of nickel |
| **7222** |  |  | **Other bars and rods of stainless steel; angles, shapes and sections of stainless steel** |
|  |  |  | - Bars and rods, not further worked than hot-rolled, hot-drawn or extruded |
| **7222 11** |  |  | - - Of circular cross-section |
|  |  |  | - - - Of a diameter of 80 mm or more, containing by weight |
| **7222 11 11** | 0.0% |  | - - - - 2.5% or more of nickel |
| **7222 11 19** | 0.0% |  | - - - - Less than 2.5% of nickel |
|  |  |  | - - - Of a diameter of less than 80 mm, containing by weight |
| **7222 11 81** | 0.0% |  | - - - - 2.5% or more of nickel |
| **7222 11 89** | 0.0% |  | - - - - Less than 2.5% of nickel |
| **7222 19** |  |  | - - Other |
| **7222 19 10** | 0.0% |  | - - - Containing by weight 2.5% or more of nickel |
| **7222 19 90** | 0.0% |  | - - - Containing by weight less than 2.5% of nickel |
| **7222 20** |  |  | - Bars and rods, not further worked than cold-formed or cold-finished |
|  |  |  | - - Of circular cross-section |
|  |  |  | - - - Of a diameter of 80 mm or more, containing by weight |
| **7222 20 11** | 0.0% |  | - - - - 2.5% or more of nickel |
| **7222 20 19** | 0.0% |  | - - - - Less than 2.5% of nickel |
|  |  |  | - - - Of a diameter of 25 mm or more, but less than 80 mm, containing by weight |
| **7222 20 21** | 0.0% |  | - - - - 2.5% or more of nickel |
| **7222 20 29** | 0.0% |  | - - - - Less than 2.5% of nickel |
|  |  |  | - - - Of a diameter of less than 25 mm, containing by weight |
| **7222 20 31** | 0.0% |  | - - - - 2.5% or more of nickel |
| **7222 20 39** | 0.0% |  | - - - - Less than 2.5% of nickel |
|  |  |  | - - Other, containing by weight |
| **7222 20 81** | 0.0% |  | - - - 2.5% or more of nickel |
| **7222 20 89** | 0.0% |  | - - - Less than 2.5% of nickel |
| **7222 30** |  |  | - Other bars and rods |
|  |  |  | - - Forged, containing by weight |
| **7222 30 51** | 0.0% |  | - - - 2.5% or more of nickel |
| **7222 30 91** | 0.0% |  | - - - Less than 2.5% of nickel |
| **7222 30 97** | 0.0% |  | - - Other |
| **7222 40** |  |  | - Angles, shapes and sections |
| **7222 40 10** | 0.0% |  | - - Not further worked than hot-rolled, hot-drawn or extruded |
| **7222 40 50** | 0.0% |  | - - Not further worked than cold-formed or cold-finished |
| **7222 40 90** | 0.0% |  | - - Other |
| **7223** |  |  | **Wire of stainless steel** |
|  |  |  | - Containing by weight 2.5% or more of nickel |
| **7223 00 11** | 0.0% |  | - - Containing by weight 28% or more but not more than 31% of nickel and 20% or more but not more than 22% of chromium |
| **7223 00 19** | 0.0% |  | - - Other |
|  |  |  | - Containing by weight less than 2.5% of nickel |
| **7223 00 91** | 0.0% |  | - - Containing by weight 13% or more but not more than 25% of chromium and 3.5% or more but not more than 6% of aluminium |
| **7223 00 99** | 0.0% |  | - - Other |
|  |  |  | **IV. OTHER ALLOY STEEL; HOLLOW DRILL BARS AND RODS, OF ALLOY OR NON-ALLOY STEEL** |
| **7224** |  |  | **Other alloy steel in ingots or other primary forms; semi-finished products of other alloy steel** |
| **7224 10** |  |  | - Ingots and other primary forms |
| **7224 10 10** | 0.0% |  | - - Of tool steel |
| **7224 10 90** | 0.0% |  | - - Other |
| **7224 90** |  |  | - Other |
| **7224 90 02** | 0.0% |  | - - Of tool steel |
|  |  |  | - - Other |
|  |  |  | - - - Of rectangular (including square) cross-section |
|  |  |  | - - - - Hot-rolled or obtained by continuous casting |
|  |  |  | - - - - - The width measuring less than twice the thickness |
| **7224 90 03** | 0.0% |  | - - - - - - Of high-speed steel |
| **7224 90 05** | 0.0% |  | - - - - - - Containing by weight not more than 0.7% of carbon, 0.5% or more but not more than 1.2% of manganese and 0.6% or more but not more than 2.3% of silicon; containing by weight 0.0008% or more of boron with any other element less than the minimum content referred to in note 1(f) to this chapter |
| **7224 90 07** | 0.0% |  | - - - - - - Other |
| **7224 90 14** | 0.0% |  | - - - - - Other |
| **7224 90 18** | 0.0% |  | - - - - Forged |
|  |  |  | - - - Other |
|  |  |  | - - - - Hot-rolled or obtained by continuous casting |
| **7224 90 31** | 0.0% |  | - - - - - Containing by weight not less than 0.9% but not more than 1.15% of carbon, not less than 0.5% but not more than 2% of chromium and, if present, not more than 0.5% of molybdenum |
| **7224 90 38** | 0.0% |  | - - - - - Other |
| **7224 90 90** | 0.0% |  | - - - - Forged |
| **7225** |  |  | **Flat-rolled products of other alloy steel, of a width of 600 mm or more** |
|  |  |  | - Of silicon-electrical steel |
| **7225 11** | 0.0% |  | - - Grain-oriented |
| **7225 19** |  |  | - - Other |
| **7225 19 10** | 0.0% |  | - - - Hot-rolled |
| **7225 19 90** | 0.0% |  | - - - Cold-rolled |
| **7225 30** |  |  | - Other, not further worked than hot-rolled, in coils |
| **7225 30 10** | 0.0% |  | - - Of tool steel |
| **7225 30 30** | 0.0% |  | - - Of high-speed steel |
| **7225 30 90** | 0.0% |  | - - Other |
| **7225 40** |  |  | - Other, not further worked than hot-rolled, not in coils |
| **7225 40 12** | 0.0% |  | - - Of tool steel |
| **7225 40 15** | 0.0% |  | - - Of high-speed steel |
|  |  |  | - - Other |
| **7225 40 40** | 0.0% |  | - - - Of a thickness exceeding 10 mm |
| **7225 40 60** | 0.0% |  | - - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7225 40 90** | 0.0% |  | - - - Of a thickness of less than 4.75 mm |
| **7225 50** |  |  | - Other, not further worked than cold-rolled (cold-reduced) |
| **7225 50 20** | 0.0% |  | - - Of high-speed steel |
| **7225 50 80** | 0.0% |  | - - Other |
|  |  |  | - Other |
| **7225 91** | 0.0% |  | - - Electrolytically plated or coated with zinc |
| **7225 92** | 0.0% |  | - - Otherwise plated or coated with zinc |
| **7225 99** | 0.0% |  | - - Other |
| **7226** |  |  | **Flat-rolled products of other alloy steel, of a width of less than 600 mm** |
|  |  |  | - Of silicon-electrical steel |
| **7226 11** | 0.0% |  | - - Grain-oriented |
| **7226 19** |  |  | - - Other |
| **7226 19 10** | 0.0% |  | - - - Not further worked than hot-rolled |
| **7226 19 80** | 0.0% |  | - - - Other |
| **7226 20** | 0.0% |  | - Of high-speed steel |
|  |  |  | - Other |
| **7226 91** |  |  | - - Not further worked than hot-rolled |
| **7226 91 20** | 0.0% |  | - - - Of tool steel |
|  |  |  | - - - Other |
| **7226 91 91** | 0.0% |  | - - - - Of a thickness of 4.75 mm or more |
| **7226 91 99** | 0.0% |  | - - - - Of a thickness of less than 4.75 mm |
| **7226 92** | 0.0% |  | - - Not further worked than cold-rolled (cold-reduced) |
| **7226 99** |  |  | - - Other |
| **7226 99 10** | 0.0% |  | - - - Electrolytically plated or coated with zinc |
| **7226 99 30** | 0.0% |  | - - - Otherwise plated or coated with zinc |
| **7226 99 70** | 0.0% |  | - - - Other |
| **7227** |  |  | **Bars and rods, hot-rolled, in irregularly wound coils, of other alloy steel** |
| **7227 10** | 0.0% |  | - Of high-speed steel |
| **7227 20** | 0.0% |  | - Of silico-manganese steel |
| **7227 90** |  |  | - Other |
| **7227 90 10** | 0.0% |  | - - Containing by weight 0.0008% or more of boron with any other element less than the minimum content referred to in note 1(f) to this chapter |
| **7227 90 50** | 0.0% |  | - - Containing by weight 0.9% or more but not more than 1.15% of carbon, 0.5% or more but not more than 2% of chromium and, if present, not more than 0.5% of molybdenum |
| **7227 90 95** | 0.0% |  | - - Other |
| **7228** |  |  | **Other bars and rods of other alloy steel; angles, shapes and sections, of other alloy steel; hollow drill bars and rods, of alloy or non-alloy steel** |
| **7228 10** |  |  | - Bars and rods, of high-speed steel |
| **7228 10 20** | 0.0% |  | - - Not further worked than hot-rolled, hot-drawn or extruded; hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 10 50** | 0.0% |  | - - Forged |
| **7228 10 90** | 0.0% |  | - - Other |
| **7228 20** |  |  | - Bars and rods, of silico-manganese steel |
| **7228 20 10** | 0.0% |  | - - Of rectangular (other than square) cross-section, hot-rolled on four faces |
|  |  |  | - - Other |
| **7228 20 91** | 0.0% |  | - - - Not further worked than hot-rolled, hot-drawn or extruded; hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 20 99** | 0.0% |  | - - - Other |
| **7228 30** |  |  | - Other bars and rods, not further worked than hot-rolled, hot-drawn or extruded |
| **7228 30 20** | 0.0% |  | - - Of tool steel |
|  |  |  | - - Containing by weight 0.9% or more but not more than 1.15% of carbon, 0.5% or more but not more than 2% of chromium and, if present, not more than 0.5% of molybdenum |
| **7228 30 41** | 0.0% |  | - - - Of circular cross-section of a diameter of 80 mm or more |
| **7228 30 49** | 0.0% |  | - - - Other |
|  |  |  | - - Other |
|  |  |  | - - - Of circular cross-section, of a diameter of |
| **7228 30 61** | 0.0% |  | - - - - 80 mm or more |
| **7228 30 69** | 0.0% |  | - - - - Less than 80 mm |
| **7228 30 70** | 0.0% |  | - - - Of rectangular (other than square) cross-section, hot-rolled on four faces |
| **7228 30 89** | 0.0% |  | - - - Other |
| **7228 40** |  |  | - Other bars and rods, not further worked than forged |
| **7228 40 10** | 0.0% |  | - - Of tool steel |
| **7228 40 90** | 0.0% |  | - - Other |
| **7228 50** |  |  | - Other bars and rods, not further worked than cold-formed or cold-finished |
| **7228 50 20** | 0.0% |  | - - Of tool steel |
| **7228 50 40** | 0.0% |  | - - Containing by weight 0.9% or more but not more than 1.15% of carbon, 0.5% or more but not more than 2% of chromium and, if present, not more than 0.5% of molybdenum |
|  |  |  | - - Other |
|  |  |  | - - - Of circular cross-section, of a diameter of |
| **7228 50 61** | 0.0% |  | - - - - 80 mm or more |
| **7228 50 69** | 0.0% |  | - - - - Less than 80 mm |
| **7228 50 80** | 0.0% |  | - - - Other |
| **7228 60** |  |  | - Other bars and rods |
| **7228 60 20** | 0.0% |  | - - Of tool steel |
| **7228 60 80** | 0.0% |  | - - Other |
| **7228 70** |  |  | - Angles, shapes and sections |
| **7228 70 10** | 0.0% |  | - - Not further worked than hot-rolled, hot-drawn or extruded |
| **7228 70 90** | 0.0% |  | - - Other |
| **7228 80** | 0.0% |  | - Hollow drill bars and rods |
| **7229** |  |  | **Wire of other alloy steel** |
| **7229 20** | 0.0% |  | - Of silico-manganese steel |
| **7229 90** |  |  | - Other |
| **7229 90 20** | 0.0% |  | - - Of high-speed steel |
| **7229 90 50** | 0.0% |  | - - Containing by weight 0.9% or more but not more than 1.15% of carbon, 0.5% or more but not more than 2% of chromium and, if present, not more than 0.5% of molybdenum |
| **7229 90 90** | 0.0% |  | - - Other |